**Nanocomposite: Synthesis and Thermal Properties of Polyaniline-Pbs using DTA Technique.**

**J. B. Bhaiswar1, S. P. Dongre2, Ravindra R.Kinge3**

1Department of Physics, Nagpur Institute of Technology, Nagpur, Maharashtra India 440022.

2Department of Physics, Bhalerao Science College Saoner, Dist. - Nagpur, Maharashtra India.441107.

3Department of Physics, Smt, .G.G. Khadse, College, Muktainagar, Dist.- Jalgaon, Maharashtra India 425306.

Email-[jitendrabhaiswar@gmail.com](mailto:jitendrabhaiswar@gmail.com),[sunildongre803@gmail.com](mailto:sunildongre803@gmail.com), [ravikinge@gmail.com](mailto:ravikinge@gmail.com)

**Abstract:**

DTA thermal analysis indicated that the Polyaniline powder had discernible moisture content. This phenomenon was in agreement with the XRD results. Moreover, in the first run of DTA thermal analysis, an exothermic peak at 150-310*o*C was found. This peak was due to the chain cross linking, resulting from a coupling of two neighboring -N=Q=N- groups to give two -NH-B-NH groups through a link of the N with its neighboring Quindío ring. Thus, on the basis of thermal profile of these materials, we can say that among all composite material, the PANI/PbS composite materials, cross-linking or oxidative reaction starts at higher temperature, which indicates that the thermal stability of PANI/PbS Nanocomposite is higher.

**Keywords:** DTA, thermal analysis, Polyaniline, Pbs, Nanocomposite

**References:**

[1]. E Peter Maziarz III; Sarah A Lorenz; Thomas P White; Troy D Wood: Polyaniline: AConductive Polymer Coating for Durable Nanospray emitters. Journal of the American Society for Mass Spectrometry **2000**, 11, 659-663.

[2]. Tiitu, M.; Talo, A.; Forsén, O.; Ikkala, O.: Aminic Epoxy Resin Hardeners as Reactive Solvents for Conjugated Polymers: Polyaniline Base/Epoxy Composites for Anticorrosion Coatings. Polymer **2005**, 46, 6855-6861.

[3]. Ismail, Y. A.; Shin, S. R.; Shin, K. M.; Yoon, S. G.; Shon, K.; Kim, S. I.; Kim, S.J.: Electrochemical Actuation in Chitosan/Polyaniline Microfibers for Artificial Muscles Fabricated using an in Situ Polymerization. Sensors and Actuators B:Chemical**2008**, 129, 834-840.

[4]. Dhand, C.; Das, M.; Sumana, G.; Srivastava, A. K.; Pandey, M. K.; Kim, C. G.;Datta, M.; Malhotra, B. D.: Preparation, Characterization and Application of PolyanilineNanospheres to Biosensing. Nanoscale**2010**, 2, 747-754.

[5]. Vibha Saxena; BD Malhotra: Prospects of Conducting Polymers in Molecular Electronics. Current Applied Physics **2003**, 3, 293-305.

[103]. Yang, Y.; Heeger, A.: Polyaniline as a Transparent Electrode for Polymer Light\_Emitting Diodes: Lower Operating Voltage and Higher Efficiency. Applied Physics Letters **1994**, 64, 1245-1247.

[6]. Pinto, N.; Johnson, A.; MacDiarmid, A.; Mueller, C.; Theofylaktos, N.; Robinson, D.; Miranda, F.: Electrospun Polyaniline/Polyethylene Oxide Nanofiber Field-Effect Transistor. Applied Physics Letters **2003**, 83, 4244-4246.

[6]. Tan, S.; Zhai, J.; Xue, B.; Wan, M.; Meng, Q.; Li, Y.; Jiang, L.; Zhu, D.:Property Influence of Polyaniline on Photovoltaic Behaviors of Dye-Sensitized Solar Cells. Langmuir **2004**, 20, 2934-2937.

[7]. Hosseini, S. H.; Oskooei, S. H. A.; Entezami, A. A.: Toxic Gas and Vapour Detection by Polyaniline Gas Sensors. Iranian polymer **2005**, 14, 333-344.

[8]. AZ Sadek; W Wlodarski; K Kalantar-Zadeh; C Baker; RB Kaner: Sensors and Actuators A: Physical **2007**, 139, 53-57.

[9]. Tsutomu Matsunaga; Hideharu Daifuku; Tadashi Nakajima; Takahiro Kawagoe:.Polymers for Advanced Technologies **1990**, 1, 33-39.

[10]. Wang, H.; Hao, Q.; Yang, X.; Lu, L.; Wang, X.: Electrochemistry Communications **2009**, 11, 1158-1161.

[11]. Kovalenko, I.; Bucknall, D. G.; Yushin, G.: Advanced Functional Materials **2010**, 20, 3979-3986.

[12]. Bła, E.; Pielichowski, J. Molecules **2006**, 11, 115-120.

[13]. Huang, X.; Wang, G.; Yang, M.; Guo, W.; Gao, H.: Materials Letters **2011**, 65, 2887-2890.

[14]. Heera, T.; Cindrella, L.:.Materials Science in Semiconductor Processing **2011**, 14, 151-156.

[15] Li, Q.; Zhang, C.; Li, J.: Photocatalysis and Wave-Absorbing Properties of Polyaniline/TiO2 Microbelts Composite by in Situ Polymerization Method.Applied Surface Science **2010**, 257, 944-948.

[16] Wang, Y.; Herron, N.: Semiconductor Nanocrystals in Carrier-Transporting Polymers: Charge Generation and Charge Transport. Journal of Luminescence**1996**, 70, 48-59.

[17]. Liu, X.-X.; Zhang, L.; Li, Y.-B.; Bian, L.-J.; Huo, Y.-Q.; Su, Z.: Electrosynthesis of Polyaniline/SiO2 Composite at High pH in the Absence of Extra Supporting Electrolyte. Polymer Bulletin **2006**, 57, 825-832.