**Optical properties of Graphene Oxide reinforced PANI/PS Nanocomposite Solution Cast Thin Films**

**Manisa Das a, IpsitaMohantyb, Udai Pratap Singh b and BibekanandaSundaraya, \***

**a** Department of Physics, Ravenshaw University, Cuttack 753003, Odisha, India

b Thin-film photovoltaic Lab, School of Electronics Engineering, KIIT University, Bhubaneswar, 751024, Odisha, India

\*e-mail: [bnsundaray@ravenshawuniversity.ac.in](mailto:bnsundaray@ravenshawuniversity.ac.in)

**Abstract**. Semiconductor band gap technology is essential in the quest to develop novel and advanced devices. Graphene-based polymer nanocomposites have recently been considered one of the most promising semiconducting materials for optoelectronic applications. In this study, camphor sulphonic acid doped polyaniline (PANI)-polystyrene (PS)-Graphene oxide(GO) composite films are prepared by the solution casting technique and are investigated by X-ray diffraction (XRD), Fourier transform infrared spectroscopy (FTIR), Transmission electron microscopy (TEM), and UV-Vis spectroscopy. The optical properties of the GO-PANI-PS polymer nanocomposite films exhibit higher refractive index (n), optical absorbance, andabsorption coefficient (α)than PANI-PS polymer matrix for UV-visible light. This is encouraging for optoelectronic applications and ultraviolet protection. Furthermore, the obtained low direct and indirect optical band gaps of the GO reinforced PANI-PS polymer nanocomposite prepared by a simple route fascinates the researchers towardsa new path for various optoelectronic applications.

References:

1. Aydin, H.;Gündüz, B.;& Aydin, C.;. Surface morphology, spectroscopy, optical and conductivity properties of transparent poly (9-vinylcarbazole) thin films modified with graphene oxide. *Synthetic Metals*. **2019**, *252*, 1-7.<https://doi.org/10.1016/j.synthmet.2019.04.002>.
2. Hurayra–Lizu, K. -A.; Bari, M. -W.;Gulshan, F.;& Islam, M. -R.; GO based PVA nanocomposites: tailoring of optical and structural properties of PVA with low percentage of GO nanofillers. *Heliyon*. **2021**, *7*(5), e06983.<https://doi.org/10.1016/j.heliyon.2021.e06983>.
3. Yahia, I. -S.;& Mohammed, M. -I.;. Facile synthesis of graphene oxide/PVA nanocomposites for laser optical limiting: band gap analysis and dielectric constants. *Journal of Materials Science: Materials in Electronics*. **2018**, *29*(10), 8555-8563.<https://doi.org/10.1007/s10854-018-8869-7>.
4. Sabry, N.; Mohammed, M. -I.;& Yahia, I.-S.;. Optical analysis, optical limiting and electrical properties of novel PbI2/PVA polymeric nanocomposite films for electronic optoelectronic applications. *Materials Research Express.* **2019**, *6*(11), 115339.<https://doi.org/10.1088/2053-1591/ab4c24>.
5. Aslam, M.;Kalyar, M. -A.;& Raza, Z. -A.;. Fabrication of reduced graphene oxide nanosheets doped PVA composite films for tailoring their opto-mechanical properties. *Applied Physics A.* **2017**, *123*(6), 1-12.<https://doi.org/10.1007/s00339-017-1035-x>.