**Synthesis, Structural and Morphological Analysis of Zn doped (WO3) Tungsten Oxide Nanoparticles**

Sarita1\*, Jagjeevan Ram2 and Mudit Prakash Srivastva1

1Department of Physics, SRM Institute of Science and Technology, Delhi-NCR Campus

2Department of Physics, Ramjas College University of Delhi New Delhi-110007

\*Corresponding Author E-mail: duhan07@gmail.com

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Abstract**

Zinc-doped tungsten trioxide (Zn-doped WO₃) nanoparticles were successfully synthesized using the co-precipitation method. The nanoparticles were prepared at varying temperatures, including room temperature, 100°C, and 400°C, to evaluate the influence of temperature on their structural and morphological properties. The synthesized nanoparticles were characterized using X-ray diffraction (XRD), scanning electron microscopy (SEM), and energy dispersive spectroscopy (EDS). XRD analysis revealed that the Zn-doped WO₃ nanoparticles exhibit a polycrystalline spherical structure with well-developed crystallinity. SEM images demonstrated that the degree of agglomeration increased significantly with a rise in synthesis temperature. This study highlights the impact of synthesis temperature on the structural and morphological features of Zn-doped WO₃ nanoparticles, providing valuable insights for their potential applications in various fields.

Keywords: Zn-doped WO₃ nanoparticles, co-precipitation, XRD, SEM, temperature-dependent synthesis.

Reference:

1. [Development of WO3-PEDOT: PSS hybrid nanocomposites based devices for liquefied petroleum gas (LPG) sensor](https://scholar.google.co.in/citations?view_op=view_citation&hl=en&user=UHfSbMMAAAAJ&cstart=20&pagesize=80&citation_for_view=UHfSbMMAAAAJ:9ZlFYXVOiuMC)J Ram et.al. J.of Materials Science: Materials in Electronics 30 (14), 13593-13603 **(2019)**
2. Enhancement of Photocatalytic and Electrochromic Properties of Electrochemically Fabricated Mesoporous WO3 Thin Films, S.-H. Baeck, et.al. Adv. Mater. 15, 1269–1273 **(2003)**
3. [Multifunctional hybrid diode: Study of photoresponse, high responsivity, and charge injection mechanisms](https://scholar.google.co.in/citations?view_op=view_citation&hl=en&user=UHfSbMMAAAAJ&sortby=pubdate&citation_for_view=UHfSbMMAAAAJ:hqOjcs7Dif8C) J Singh et.al., Journal of Applied Physics 123 (17), 174503 **(2018)**
4. Chandramohan R,Vijayan T A,Arumugam S,Ramalingam H B,Dhanasekaran V,Sundaram K, Mahalingam T, Effect of heat treatment on microstructural and optical properties of CBD grown Aldoped ZnO thin films, Materials Science and Engineering:B, 2011, 176, 152–156.
5. Bacaksiz E, Aksu S, Yılmaz S, Parlak M, Altunbaş M, Structural, optical and electrical properties of Al-doped ZnO microrods prepared by spray pyrolysis, Thin Solid Films, 2010, 518 ,4076–4080.
6. Dghoughi L, Ouachtari F, Addou M, Elidrissi B, Erguig H, Rmili A. Bouaoud A, The effect of Aldoping on the structural, optical, electrical and cathode luminescence properties of ZnO thin films prepared by spray pyrolysis, PhysicaB, 2010, 405,2277–2282.